

TPM update SOP


1. Extract DTPMFWUpdate.zip and copy all file to Shell bootable USB disk.




2. Insert the WINPE x64 USB disk in the machine.

3. Power on the machine, press F2 until enter BIOS Setup, then go to the Main Tab, enable F12 Boot Menu and save the configuration. Press F10 save the configuration and exit, the machine will reboot automatically.





4. During the reboot, press F12 until enter Boot Manager, it will show as picture below:



5. Select your USB bootable device, then enter to its Shell environment.

6. Select USB diskpart and then enter into DTPMFWUpdate tool path run TPMFWUpdate.nsh

After return success reset the units.

