

**Steps:**


1. Make sure adapter has been connected before executing ME update executable file. Take "SFL140M2\_MTU\_Update ME.exe" as an example
2. Open the ME-Read document and run "me-read.bat" with administrator privileges




1. In the pop-up window, view the previous version of ME FW: 18.0.5.2062




1. Double-click "SFL140M2\_MTU\_Update ME.exe" and click "Run" after the pop-up window.



1. After the Warning pop-up, click "yes" and the update will start running





1. After the update is complete, the system automatically restarts. Run “me-read.bat” again to check the updated ME FW version: 18.0.10.2269

