Synaptics Driver Release Notes for acer
OS: 32-bit and 64-bit Windows 7, Windows 8, Windows 8.1 and Windows 10
Languages Supported: English, Arabic, Portuguese (Brazil), Croatian, Czech, Danish, French, French Canadian, Finnish, Greek, German, Hungarian, Indonesian, Hebrew, Italian, Japanese, Korean, Spanish (Mexico), Dutch, Norwegian Bokmal, Polish, Portuguese, Romanian, Russian, Swedish, Slovakian, Spanish (Spain), Slovenian, Thai, Turkish, Traditional Chinese, and Simplified Chinese.
Version: 19.0.9.22 Date: 03-18-2016

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-32611 | PNPID request : inf : acer.inf ; | add new pnpid for acer
HDR-32653 | Pinch gesture doesn't smooth on the MS photo viewer | acer.inf | Adjust pinch speed(speed up).
HDR-32654 | Scrolling gesture doesn't smooth(horizontal) and delay | acer,inf | Enable scrolling inertia by default

Version: 19.0.9.21 Date: 10-06-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-31189 | [Acer/Wistron] change the pointer to 200 as default | SetMotionSpeed.reg | Change pointer motion speed to 512

Version: 19.0.9.20 Date: 09-14-2015
System enhancements
Version: 19.0.9.19 Date: 09-11-2015
System enhancements
Version: 19.0.9.18 Date: 09-07-2015
System enhancements
Version: 19.0.9.17 Date: 09-04-2015
System enhancements
Version: 19.0.9.16 Date: 09-02-2015

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Merge settings for rotating with win10 photos app into branch_v19_0_9_main_branch

Version: 19.0.9.15 Date: 08-21-2015
System enhancements
Version: 19.0.9.14 Date: 08-17-2015
System enhancements
Version: 19.0.9.13 Date: 08-17-2015
System enhancements
Version: 19.0.9.12 Date: 07-28-2015
System enhancements
Version: 19.0.9.11 Date: 07-27-2015
System enhancements
Version: 19.0.9.10 Date: 07-01-2015
System enhancements
Version: 19.0.9.9 Date: 06-26-2015
System enhancements
Version: 19.0.9.8 Date: 06-15-2015
System enhancements
Version: 19.0.9.7 Date: 06-15-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29556 | Some driver features (2 finger tap) are not work by default, when we install acer driver in windows 10 PS2 system | We should back compatible with the win8 settings when OS is windows 10 in kernel

Version: 19.0.9.6 Date: 06-11-2015
System enhancements
Version: 19.0.9.5 Date: 05-29-2015
System enhancements
Version: 19.0.9.4 Date: 05-27-2015
System enhancements
Version: 19.0.9 Date: 05-21-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-29353 | Change featurescore to 0xF9 per MS recommendation | Changed FeatureScore to 0xF9
|  | Update DriverName to the one with UUID appends.

Version: 19.0.8 Date: 05-14-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-10618 | SynCOM samples have errors and warnings when compiling | mfctest; keypad; cPadClock; cPadImage; Disabler; Comtest; DisableGesture; SynDrumPad; BezelTest; SynWrapSample; SynPlot; SynDrumPad take out from SDK since it depends srd party library DirectX; SynView; SynForcePad; Dpn't include build bat files
HDR-13375 | Remove LAPACK copyright info | Copyright 2014 to 2015; Remove LAPACK copyright info
HDR-28137 | Un-installation driver is not clean | Use %ProgramFiles%\Synaptics\SynTP as temp dir to install auxiliary drivers instead of creating temp dirs in %ProgramData%
HDR-29104 | Change driver package name from SynARP | Update OS support information in SynPD.inf
HDR-26997 (FM: 2259) | This is a placeholder for build generated checkins. | Update ReleaseNotes.html

Version: 19.0.7 Date: 05-08-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28137 | Un-installation driver is not clean | Un-installation driver is not clean - remove old SynTPCoInstaller; Use %ProgramFiles%\Synaptics\SynTP as temp dir to install auxiliary drivers instead of creating temp dirs in %ProgramData%; Always overwrite Coinstaller in update install
HDR-28874 | Incorrect ASIC Displayed in Diagnostics Window | Get correct ASIC type from F01 query 19.
HDR-29080 | Suppress Tap on Top Left Corner for SecurePad | Added code to suppress tap in the SecurePad notch area.; Checked whether query41 exists to find right offset for query43.
HDR-29102 | Update control panel to disable top left corner tap zone from UI | Hidden top left tap zone controls from the control panel.; Fixed a compiling error.
HDR-29103 | Update device type to SecurePad for SecurePad in the CPL to refer the device type | Updated device type to SecurePad in the CPL to refer the device type for SecurePad

Version: 19.0.6 Date: 04-30-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28622 | Tap zones can't work on the top right and top left corner | Allowed tap if a finger is in tap zone and object type is non-finger and tap zone is enabled.
HDR-28913 | Return code=-1 | Fixed return code for setup

Version: 19.0.5 Date: 04-23-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28907 | Correct Finger Packet State not for all fingers in a group but for those who are really in the zones | Correctly update Finger Packet State not for all fingers in a group but for those who are really in the left/right/resting zones
HDR-28944 (676644) | [Microsoft Windows 10 Team] [DeviceCompat][HID][CUET] : The check box setting "Disable internal pointing device..." in mouse properties under clickpad tab doesn't get applied. | Fixed checkbox out of sync issue when there are two tabs in the control panel such as Show tray icon in the taskbar or disable internal pointing device when external USB pointing device is attached.

Version: 19.0.4 Date: 04-16-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28831 | PNPID Request: 1B8A,1B8B,1A8C Inf: Acer | Add new pnpid for acer

Version: 19.0.3 Date: 04-09-2015
System enhancements
Version: 19.0.2 Date: 04-02-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28731 | Add FeatureScore for all OEM INFs. | Fixed build errors.; Added FeatureScore in INF so OEM driver is always picked by WU first so the generic driver can be overridden in WU.
HDR-28736 | Change SMBus mode switch retry to zero | Removed SMBus mode switch retry from SwitchMode because there is a retry logic in the low level driver (retry 16 times).

Version: 19.0.1 Date: 03-26-2015
System enhancements
Version: 19.0.0 Date: 03-19-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28484 | Create miniport driver INF for major customers. | Created miniport driver installation package for major ciustomers. 1, Added plugin registries back fir miniport driver, otherwise synthenh cannot be launched. 2, Always created OSD class instead of enabling by registry because OSD is used several placec, if this registry is missing, the syntpenh will crash.
HDR-28488 | Gesture and Pointing performance improvement | 1, Fixed memory leakage when the miniport driver is disabled or removed. 2, Fixed the miniport driver is disabled when any USB mouse is unplugged from USB ports. 3, Reported to PTP using normalized X, Y instead of filtered X, Y.; Fixed 1palm+1F failure issue if palm is down first, 1F is down second, then palm is up, the pointing does not work any more. We should fill in finger data one by one from array index 0, should no gap between finger data..

Version: 18.2.3 Date: 03-12-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28484 | Create miniport driver INF for major customers. | Created miniport driver installation paclage for major ciustomers.

Version: 18.2.2 Date: 03-06-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28341 | Review all INFs to add HID/ACPI before PnP IDs | Per Win10 WU we have to add ACPI before PnP IDS isntead of *.
HDR-28359 | PNPID Request: 1B89 Inf: Acer | Add new pnpid for acer (win7 ps2 for hw id: 1B89)

Version: 18.2.1 Date: 02-27-2015

Issue Number | Description | Fix Comment
--- | --- | ---
PRJ-35549 | Find a solution to enable SMB driver update for specific PnP in WU | Enable SMB driver update for specific PnP in WU

Version: 18.2.0 Date: 02-19-2015
System enhancements
Version: 18.1.53 Date: 02-12-2015
System enhancements
Version: 18.1.52 Date: 02-05-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28175 | Hide all edge swipe controls for Win10 | Hidden edge swipe controls from CPL for Win10.
HDR-28189 | Add Intel SkyLake chipset support in SMB INF | Added Intel Skylake chipset support for SMBus.

Version: 18.1.51 Date: 01-29-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28093 | PNPID Request: 1B87 Inf: Acer | Add new pnpid
HDR-28112 | PNPID Request: 1B88 Inf: Acer | Add new pnpid

Version: 18.1.50 Date: 01-22-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28039 | TouchPad should be enabled after checked "Disable internal pointing device when external USB pointing device is attached" then unplugged external USB mouse. | Fixed the USB mouse plugin/unplugin disable/enable issue, the notification reason is changed, it does not match with user mode driver, so the event is not processed by the user mode driver.,
HDR-27998 | PNPID Request: 1B86 Inf: Acer | Add new pnpid

Version: 18.1.49 Date: 01-15-2015
System enhancements
Version: 18.1.48 Date: 01-08-2015

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-27930 | Disable audio feedback for button clicking | Read ForcePad click sound mute status from registry..
HDR-27895 | PNPID Request: 1B83 Inf: Acer | Add Pnpids (1B83, 1B84, 1B85) for win7
HDR-27896 | PNPID Request: 1B84 Inf: Acer | Add Pnpids (1B83, 1B84, 1B85) for win7

Version: 18.1.47 Date: 12-25-2014
System enhancements
Version: 18.1.46 Date: 12-18-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-913 (Hyder001) | Using force data to reduce false taps working with ACM | Ignored tap decoding if force is less than certain threshold.

Version: 18.1.45 Date: 12-11-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-27746 | Add more log information in the driver | Logged ForceModel reset event.

Version: 18.1.44 Date: 12-05-2014
System enhancements
Version: 18.1.43 Date: 11-26-2014
System enhancements
Version: 18.1.42 Date: 11-20-2014
No changes
Version: 18.1.41 Date: 11-14-2014
No changes
Version: 18.1.40 Date: 11-07-2014
No changes
Version: 18.1.39 Date: 10-31-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-626 (ECR232511) | Unqouted Service Path in Registry with SynTPEnhServic | add quotes to Service's ImagePath in Registry

Version: 18.1.38 Date: 10-24-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-624 | Make DPI aware default disabled | Make DPI aware
HDR-65 | TouchPad doesn't work for a time after detaching external USB mouse | Fixed TouchPad does not work after detaching external mouse
HDR-513 | PNPID Request: 1B81 Inf: Acer | Add new pnpid 1B81 (HID/I2C + PS2 PTP)

Version: 18.1.37 Date: 10-17-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-511 | Pinch does not work in ForceTutorial app | Fixed wrong cursor position when DPI aware is enabled in syntpenh, that caused pinch or scrolling does not work if it uses wheel mouse message and the system is not in 96dpi. Called right function to window handle under pointer to fix wrong window handle which causes pinch does not work in ForcePad Tutorail app.

Version: 18.1.36 Date: 10-09-2014
No changes
Version: 18.1.35 Date: 10-02-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-28 | [3+2BCP] 3F swipe not working on Metro Photo Application | Make 3F swipe working in Metro Photo Application
HDR-411 | Powerpoint 2013 will be Grayed when using finger to Horizontal scrolling | Used key scroll instead of bar scrolling for PowerPoint to fix "Powerpoint 2013 will be Grayed when using finger to Horizontal scrolling".

Version: 18.1.34 Date: 09-25-2014
No changes
Version: 18.1.33 Date: 09-18-2014
No changes
Version: 18.1.32 Date: 09-11-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-264 | Audio feedback missed if clicking is too fast and audio playback is too slow | Queued clicking press/release event, then playback audio feedback one by one if the queue is not empty, this fixed clicking sound missing or press/release misorder.

Version: 18.1.31 Date: 09-04-2014

Issue Number | Description | Fix Comment
--- | --- | ---
HDR-208 | Remove allowing edge swipe if first three packets are palm | Removed old implementation for relaxing palm rejection in the edge fro edge swipe gestures.
HDR-209 | Add API to disable/enable suppression motion while typing. | Exposed API to allow an application to disable/enable motion suppression while typing.
HDR-210 | Force drag is triggered unexpected | Fix an wrong ForceReleased drag generated by Force-Clciking-releasing without motion before release force.
HDR-227 | Relax edge swipe condition in edge if first three packets are palm | Ignored palm check for first three packets if it is edge swipe, this will fix edge swipe missing with large flat finger or very fast edge swipe.
HDR-189 | acer ZQM: PS2 driver request in win8.1 | Remove the unnecessary changes in last check-in.
HDR-189 | acer ZQM: PS2 driver request in win8.1 | Add PS/2 driver support for SYN1B7C and SYN1B7D in Win8.1.

Version: 18.1.30 Date: 08-29-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | "Enable" button is not greyed out if the TP is disabled, then plug in USB mouse with "Disable internal pointing device when external USB pointing device is attached" checked.

Version: 18.1.29 Date: 08-21-2014
No changes
Version: 18.1.28 Date: 08-15-2014
No changes
Version: 18.1.27 Date: 08-07-2014
No changes
Version: 18.1.26 Date: 08-01-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48511 | Project: ZQM, Request Win8.1 PS2 driver; could not install the driver Win8.1 PS2 mouse device.HWID: SYN1B7B | Add PS/2 driver support for SYN1B7B in Win8.1.

Version: 18.1.25 Date: 07-25-2014
No changes
Version: 18.1.24 Date: 07-17-2014
No changes
Version: 18.1.23 Date: 07-10-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47650 (ECR209588 -> Win7, ECR209586 -> Win8) | UI translation on Chinese Simplified | New translations for the word "Charms" for Windows 8
TP-48348 | SynTPEnh crashes when the driver is uninstalled. | Fixed syntpenh crash when the dirver is uninstalled.

Version: 18.1.22 Date: 07-04-2014
No changes
Version: 18.1.21 Date: 06-26-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48242 | Remove all short cuts all user when the driver is uninstalled/upgraded. | Remove All users short cuts in uninstallation or before driver update

Version: 18.1.20 Date: 06-20-2014
No changes
Version: 18.1.19 Date: 06-12-2014
No changes
Version: 18.1.18 Date: 06-06-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-48043 | Add TM number in configkey | Appended TM number in configkey so we can support multiple TouchPad in the system.

Version: 18.1.17 Date: 05-29-2014
No changes
Version: 18.1.16 Date: 05-22-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47648 (ECR209588 -> Win7, ECR209586 -> Win8) | UI translation on Brazil Portugese | Fix Portuguese translation for "charms" from Windows 8
TP-47650 (ECR209588 -> Win7, ECR209586 -> Win8) | UI translation on Chinese Simplified | Add translated strings for TouchPad Pointing Speed and 3F Swipe; Fix Traditional and Simplified Chinese words for Win8 Charms
TP-47856 | Text "Momentum" is not translated | Restore translation for "Momentum"
TP-47874 | SynForcePad is not working on SMB or HID/I2C system | Modified the connection type in SynForcePad so we can run the demo app on SMB and other platform.

Version: 18.1.15 Date: 05-15-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47801 | On simplified Chinese language, the translation for "Pointing Speed" is different from the help file on the General tab | Fix Traditional Chinese translation for "Pointer Speed" help topic
TP-47860 | Spell out FW to Firmware | Spelled out FW VErsion to Firmware Version.

Version: 18.1.14 Date: 05-09-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47799 | Set focus on Synaptics device tab | Set focus to Synaptics tab after the CPL is opened.
TP-47814 | Top edge zone size is wrong | Top edge swipe zone size is wrong, whole TP is top edge swipe zone, this causes tue cursor cannot be moved vertically.
TP-47815 | Change FW version display format for HID device | Changed FW version display format for HID device from major.minor to an integer.

Version: 18.1.13 Date: 05-01-2014
No changes
Version: 18.1.12 Date: 04-25-2014
No changes
Version: 18.1.11 Date: 04-18-2014
No changes
Version: 18.1.10 Date: 04-10-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Fixed TP lost function after this power sequence s3->s4->resume.resume from s4, then resume

Version: 18.1.9 Date: 04-03-2014

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Prevent unnecessary registry reads if stick device is not present.
TP-47221 | Cursor gets stuck inside Application's border | Fixed "Sticky Border" option (in Accessibility options) so that the cursor is not stuck inside application's border after the application is closed.

Version: 18.1.8 Date: 03-27-2014
No changes
Version: 18.1.7 Date: 03-21-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46951 | Remove setting remote control region register for AMD SMB driver | Don't touch other bits of ASF_IO index 0x15 register, otherwise ASF does not work after S3/S4/S5.
|  | Added button state in packet when momentum was stopped otherwise drag was dropped after momentum if the button is still down.
|  | Greyed out some controls in main page if the device is disabled.

Version: 18.1.6 Date: 03-13-2014
No changes
Version: 18.1.5 Date: 03-06-2014
No changes
Version: 18.1.4 Date: 02-27-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-47170 | customer report filter activation time is in 0/6, correct setting should be in 2/6 | Modified PalmCheck filters registry path to get settings for either ACM1 or ACM2.0.; Set advanced filter timeout to notch 2 (1sec).

Version: 18.1.3 Date: 02-21-2014
No changes
Version: 18.1.2 Date: 02-13-2014
No changes
Version: 18.1.1 Date: 02-07-2014
No changes
Version: 18.1.0 Date: 01-30-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46951 | Remove setting remote control region register for AMD SMB driver | Removed unnecessary code to change the slave address of AMD SMB controller1 for ASF, this caused NIC fails to talk with SMB ASF.

Version: 18.0.9 Date: 01-23-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46856 | Turn on Enhancement service for acer and acer_RMIHID INFs | Use SynTPEnhService to launch enhancement for acer and acer_RMIHID
TP-46858 | PnP ID Request for Wistron/Acer | Pnpid request 1B7F (copy 1B76). Wwindows7, windows8.0 use acer inf, and windows8.1 use acer_RMIHID inf.
TP-46859 | PnP ID Request for Pegatron/Acer | Pnpid request 1B80 (copy 1B66). Wwindows7, windows8.0 use acer inf, and windows8.1 use acer_RMIHID inf.

Version: 18.0.8 Date: 01-16-2014
No changes
Version: 18.0.7 Date: 01-10-2014

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46476 | [ACM2.0] Edge swipes | Eliminated accidental edge swipe while a finger moved to edge area of TouchPad.
TP-46588 | New Video for SGS94 and UX_UI | Updated Control Panel Help Video files.
TP-46749 | Improve 2F scrolling and inertial by using history data | Remove flag that is no longer used. Improve scrolling and inertia by using history data. Update 2FScrolling inertia settings for improved 2F scrolling. Change Inertia speed to be consistent with current settings.

Version: 18.0.6 Date: 12-27-2013
No changes
Version: 18.0.5 Date: 12-20-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46624 | Suppress Palm Clicking for ForcePad | Suppressed palm clicking for ForcePad.

Version: 18.0.4 Date: 12-12-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46277 | Pinch has low trigger rate | Forget to merge the correct setting and remove the image capability, it causes the touchpad behavior not correct.

Version: 18.0.3 Date: 12-06-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Lower the warning level to avoid annoying debug message.
TP-46526 | Unexpected Click when a finger moves out of TouchPad from edge | Fixed unexpected click when a finger moves out of the ForcePad from edge.

Version: 18.0.2 Date: 11-27-2013
No changes
Version: 18.0.1 Date: 11-21-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46377 | Change right edge swipe setting on SYN1B79 | Adjust right edge swipe zone size.

Version: 18.0.0 Date: 11-14-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46243 | Difference performance of 2 Finger Tap | Wait 20ms delay and retry ModeSwitch until it is sucessful or timeout.

Version: 17.1.1 Date: 11-07-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46162 | HP-_project_: Unable to set EdgeMotion Speed faster than default | Increased maximum edgemotion speed which has more selections from the edge motion speed slider.
TP-46206 | Locking Drag has no function in OEM INF | Fixed Lock Drag no funtion issuel.
TP-46218 | Calculate the force after TPFiler | Calculate the force after TPFiler
TP-46220 | Make ClickDrag edgemotion on ForcePad | Made ClickDrag edgemotion work after force calculation was moved after CTPFilter.

Version: 17.1.0 Date: 10-31-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45899 | Add Code for supporting Legacy TouchPad PC settings opt-in on win 8.1 | Add code to support Legacy touchpad setting on win8.1
TP-45967 | BSOD on version 17.0.8.11 | Check IRQL before calling KeClearEvent.
TP-46066 | 2F click & drag terminates when the force is relaxed = make it similar to 1F click & drag | Added code to support 2F drag with force released.
TP-46082 | BSOD after S3 resume | Move startTimer in front of syn function.

Version: 17.0.20 Date: 10-25-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-46014 | OEMWPF and OEMWPF_RMIHID: TP can't work after drag file with DragLock function enabled with TP v17.0.17.0 | Added fix to release drag lock after 500ms timeout, and not make touchpad frozen. Update code to allow dribble packets to be sent, but not mess other sending group packets.
TP-46095 | Implement scan code for Touchpad on off control and 97 commands on SYN1B6F | Add scan code enable/disable touchpad and KBC Notification when enable/disable touchpad for PNPID 1B6F; Fix inf build error

Version: 17.0.19 Date: 10-17-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45281 | Click action is not consistent | Fixed the issue which checked wrong registry control for enabling/disabling 1Palm+MF clicking.
TP-45755 | resting palm + 1F click or 2F click support | Removed TL2s.
TP-45976 | Skip force calculation for Palm | Skipped force calculation if there is only palm without any finger.

Version: 17.0.18 Date: 10-11-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45934 | Add different force release threshold for 2F drag there is one finger in the button | Added another force release threshold for 1F resting + another finger drag.
TP-45976 | Skip force calculation for Palm | Skipped force calculation for palm object.; Skipped force calculation if there is only palm without any finger.
TP-45977 | Add "Enable Force" in the tray icon to disable/enable force continuation. | Added control option "Enable Force" in tray icon that allows end user to enable/disable force conitnuation pinch and scrolling, and 2F clicking.

Version: 17.0.17 Date: 10-03-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45281 | Click action is not consistent | Added registry control to enable/disable 1Palm+MF clicking.
TP-45755 | resting palm + 1F click or 2F click support | 1, Used ClickSmart for 2F click in ForcePad, we don't need to consider the force. 2, Made 1Palm+1F and 2F click work.
TP-45756 | resting palm + 2F tap | Fixed bit mask. Reimplemented MF tap with resting fingers in button zone.
TP-45918 | Add FW RawPacket Position filter to the driver | Add FW RawPacket Position filter to the driver
TP-45891 | Change driver setting | Remove KBC Notification (97 command)

Version: 17.0.16 Date: 09-26-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44750 (20130628 meeting with Kirk) | After log file capture Kirk would like the default folder opened so that the log file can be copied or viewed instead of just closing | Add option for user to open log file folder after collecting diagnostic info
TP-45827 | Add option to show progress either in current command prompt window or show it in another command prompt window title | Added an option to show progress either in current command prompt window or show it in another command prompt window title
TP-45839 | 2F horizontal scroll will flip over two pictures on Windows Photo viewer and Acer Photo | Remove 2 finger horizontal scroll for all photo apps and add Acer Photo app specific settings for rotation and 3 finger flick

Version: 17.0.15 Date: 09-19-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Added HID mouse filter callback functions.
TP-45582 | BSoD on WHCK test | Keyboard filter driver should pass specific IOCTL to function driver.
TP-45786 | BSOD 0x1E occur when customer uninstall driver | For uninstall case, we still need to unregister notification handler.
TP-45792 | 988033 Touchpad cannot be disabled/Enabled by hotkey(Fn+f2)on bullet unit | Fix Mux KBC if touchpad is connected to port 1, 2 or 3.
TP-45801 | Keep motion/tap/gesture suppression after palm before timeout | Last palm time stamp variables were reset. Fix "keep motion/tap/gesture suppressed after palm before timeout" feature.
TP-45803 | Show right asic type from Diag. page | Show right ASIC type for 1320 and 1321 on Diag. page.
TP-45769 | Top Edge Pull won't work on Metro style Camera and Photo, after fix TP-44956 | fix top edge pull doesn't work on metro camera and metro photo.

Version: 17.0.14 Date: 09-13-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45582 | BSoD on WHCK test | Fix BSOD when doing system WHCK test
TP-45663 | BSOD for WHCK "Fault Injection Test" | Fix WHCK Fault Injection Test
TP-45657 | Short finger moving would cause tap | Shorten the finger movement delta of a tap
TP-45658 | Add MS word to ZoomPerfect supporting app list | Add Microsoft Word to zoom-perfect support list (enable touch-injection for edge swipe, 2 finger scroll, pinch)
TP-45711 | Change SYN1B6F to SMBus mode from PS/2 as default | Change SYN1B6F setting to InterTouch from PS/2

Version: 17.0.13 Date: 09-05-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44637 | Testarossa - BITS087995: [PT_TSA]Sometimes mouse cursor don't change icon as scrolling | Added fix to show custom cursor correctly.
TP-45194 | English description on Simplified Chinese OS | Update translations
TP-45590 | BSOD 0x10D occur when doing Restart,S3 and S4 +LAN (Right usb port) 14 hours | Unregister RMI callback func before register it.
TP-44486 | 4 Corner Tap Fail in acer.inf | Solve corner tap with smart-sense enabled (edge tap starting zone) in profile sensor system. We force to trigger corner tap action even when edge-tap violation occurs.

Version: 17.0.12 Date: 08-30-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45504 | Spyder ULT - There is no function after install driver | Pass the WdfRequest handle to the WDF function .
TP-44956 | Win 8.1 issue - Touchpad 2F horizontal scrolling speed too fast on metro app Photos and Camera | Customer requests to force disable Inertia in metro camera app for 2 finger horizontal scrolling
TP-45379 | Win 8.1 issue - 3F press function has high fail rate | Fixed the high fail rate of Three finger press.

Version: 17.0.11 Date: 08-23-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45258 | OEM_project_ (SYN1E62) - BSOD after installing v17.0.9 driver | Use InterlockedExchange() and add comments.
TP-44486 | 4 Corner Tap Fail in acer.inf | For image sensor touchpad, corner tap still has response even if smart sense tap starting zone is enabled. Add image sensor capability for all system to make them behave the same.
TP-45384 | Default button did not work | Fixed default button does not work for ZoomPerfect

Version: 17.0.10 Date: 08-15-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45096 | Device fails detection after reflashing fw using SynapticsReflash found in v17_0_7 | Fixed Device fails detection after reflashing fw
TP-45258 | OEM_project_ (SYN1E62) - BSOD after installing v17.0.9 driver | Use atomic variable to avoid reentry and add timeout mechanism as well.
TP-44956 | Win 8.1 issue - Touchpad 2F horizontal scrolling speed too fast on metro app Photos and Camera | Fix typo

Version: 17.0.9.1 Date: 08-14-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45258 | OEMEnvy (SYN1E62) - BSOD after installing v17.0.9 driver | Rollback codes. It seems problem to call Mutex acquire function in DPC.

Version: 17.0.9 Date: 08-08-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-45025 | After use touchpad to reboot system, it would BSOD in OS | Check IRQL before calling RtlQueryRegistryValues function.
TP-45111 | Mode switch failed on Win8.1 | Suppor OEM SMBus Host Controller.
TP-45147 | Cusor jumps with OEM 5BFP | Add mechanism to avoid reentry for SMBus driver. Port reentry avoidance mechanism to CRMIPort.

Version: 17.0.8 Date: 08-01-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-42303 | Improve Driver build process and release note for customers | Remove useless notification in middle of build; Fix file verification script; Fix UTF-8 failure to translate non-ASCII apostrophe in release notes
TP-44354 | Horizontal two finger scrolling can't work on PDF file via win8 PFD APP | Fix horizontal scrolling becomes vertical scrolling in Metro simple Chinese pdf reader
TP-44770 | Bonsai - Can not use zoom in/out function after put a third or more fingers on the touchpad | Avoid canceling pinch action when more finger down feature is set.
TP-44975 | WHCK Failure (PS/2) - 17.0.5.3 | HPConsumer.inf (Next/Blue) | Added Synaptics generic compatible ID *SYN0002 for all PS2 touchpad infs; Added a hack until Microsoft fixes its WHCK tool
TP-45042 | Scrolling is not smoothly on metro app Photos and Camera while ZoomPerfect is enabled | Fix injection error for 2 finger scrolling gesture under Metro-mode app. This error will cause scrolling not smooth.
TP-45019 | 2F scrolling would fail or not smooth sometimes | Don't use touchinjection for 2 finger scrolling and rotation gesture in desktop mode IE.
TP-45065 | Install SMBus driver for Win7 | Add SMBus driver for all Acer INF.

Version: 17.0.7 Date: 07-26-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44571 | Spyder ULT - Default setting is incorrect | Duplicate of ClickpadViews, ClickpadViewModel for OEM Win7 UI for 2013.
TP-44879 | OEMWPF TPPB - modified Win7 UI for 2013 | Changed help text. Added new help text, all in English for now.

Version: 17.0.6 Date: 07-18-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Display ACM 2.0 type in Diagnostic panel
TP-44941 | Getting wrong register offset of ACM20 existence for old FW | Parsing ACM2.0 existence information correctly.; Update the packrat number.; Provide ACM2.0 disabled setting.
TP-44928 | Change the behavior to make 2F scrolling function on Photo Viewer | When photo app is on the foreground, 2 finger vertical scroll should work as normal.

Version: 17.0.5 Date: 07-11-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Follow-up: add registry overrides for RMI4 caps; Add RMI4 capabilities query to API
TP-44188 | Customer wants previous release notes combined with current release notes | Add a "history" feature to ReleaseNotes.HTML; Build script now creates a history from previous release notes
TP-44828 (958966) | It will pop up the error "SynTPEnh.exe-Entry Point Not Found" at the end of insttalling Synaptics driver on Vista 32&64. | Fixed SynTPEnh and SynTPHelper crash in Vista with driver built with Vs2012

Version: 17.0.4 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
|  | Do fixme and handle F11 data offsets properly. Still a wip since a large number of F11 data registers remain unchecked in the interrupt handler.
TP-44721 | Geasture issue on Google Chromewith High DPI setting | Fixed issue of two finger scrolling not working when cursor is near the right edge of the window with DPI=150%
TP-44750 (20130628 meeting with Kirk) | After log file capture Kirk would like the default folder opened so that the log file can be copied or viewed instead of just closing | In Windows 8.1 Preview, the GetVersion(Ex) APIs have been deprecated.; In Windows 8.1 Preview, the GetVersion(Ex) APIs have been deprecated. Update Manifest

Version: 17.0.3 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-42303 | Improve Driver build process and release note for customers | For release notes, if "Contact" field is missing, print the Creator of the Jira issue; Create a default empty dictionary in case JSON load fails for invalid and missing Jira numbers; Use Python decode('utf-8-sig') to strip byte order mark out of text; Do not distribute Release.txt any more since it is not updated. Use ReleaseNotes.html.
TP-43964 | ACM 2.0 change of algorithm strength driver meta-bug | Make contact type interface consistent. Add HasACM2() query.
TP-44618 (TM-2768-001) | The systray icons will flicker when scrolling in a photos viewer with three finger flick | Only turned on IME workaround for twist action instead of all gestures for Photo Viewer.
TP-44682 | Use maximum force instead of total force for multiple fingers click | Used maximum force instead of total force for MF click.
TP-44692 (ECR177029, ECR176429) | Copyright issue | Update Coypyright to 1996-2013
TP-44541 | Cursor could not move while typing | Don't suppress cursor in active area, even near key press. Only suppress gesture and tap for whole touchpad when near key press. And also enable starting zone after key press.
TP-44654 | Add ZoomPerfect feature and related settings to SYN1B79 | add ZoomPerfect feature and related settings to SYN1B79 for win8 system

Version: 17.0.2 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44299 | Right side, down side "Return at edge of screen" in Momentum doesn't work | Fixed the bounce off screen edge in momentum not working issue with high DPI.
TP-44543 | It would easily fail if doing 2F scrolling and then pinch quickly | Remove bcfeRestrictTo2FLinearScrollWhileInertia, because it often causes doing pinch gesture after doing 2 finger scrolling gesture triggers 2 finger scroll action.

Version: 17.0.1 Date: 07-10-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44440 | Convert packet count to time | Improve taps-Convert packet count to time.; Make gesture work properly for different report rates of devices; Make PalmOnPad gesture works normal for various report rate of devices.; code improve by rename a function.; Add a utility function to clear packet.
TP-44531 | Silent Uninstallation fail in in toshiba.inf | Silent Uninstallation fail with SynIsdll built with Vs2012; Silent Uninstallation fail in in Win8 x64
TP-44533 | Application crashes when we double tap on the top left corner of the TP to disable the touchpad in HPNEWUI v17.0.0 | Changed call convention from std to cdecl to fix syntpenh creash when it reads Png file.
TP-44564 | ACM2.0 can't work on OEM machine | FollowUp:Change uiQuery36Offset -- to uiQuery36Offset--.; Correct RMI query parsing.
TP-44542 | No up/down selection for right edge swipe | Remove right edge swipe up down and selection action.

Version: 17.0.0 Date: 06-07-2013

Issue Number | Description | Fix Comment
--- | --- | ---
TP-44045 | _project_ (175) - Tap to click will invalid for few seconds after 2 or 3 finger slide on pad | Improve conmunication between API and Kernel Driver.;
TP-44046 | _project_ (176) - Continue tap the 2-finger on the touchpad surface will always trigger both of mouse right and left button events. | Improve tap vs drag with 1F and multifingers, as well as communication between API and Kernel Driver..
TP-44244 | Task tray Synaptics icon, "Pressure graph" and "MoodPad" items cannot be seen. | Fixed the wrong location of popmenu by right clicking trayicon, when the size of all items is set to 150% in control panel.
TP-44299 | Right side, down side "Return at edge of screen" in Momentum doesn't work | Fixed the bounce off screen edge in momentum not working issue, when the size of all items is set to 150% in control panel.
TP-44300 | Enable Tap zone, even touch right up corner, Maximum windows doesn't work | Fixed the issue of maximizing windows not working, when the size of all items is set to 150% in control panel.
TP-44348 | Switch from VS2005 to VS2012 by Default | Save 2005 solution; Switch from VS2005 to VS2012 by Default Use include and lib files from T drive; Bump SynTPCo19.dll to SynTPCo20.dll; SynDell;share\Png; Solution files; KmdfLibraryVersion = 1.11, WdfCoInstaller01011.dll; SynOsLib dir.lst; Remove ...2012.sln files; Inf2Cat; forcetext2bin; Use Include and lib files from T drive
TP-44457 | 16.6.5 sony2006.inf Two-Finger horizontal scroll failed. | Only read application specific settings when apps switch happens, otherwise some user specific settings will be overridden if CPL is opened and changes are not apllied.