

# Steps:

1. *Copy the file "AL156P1\_JL\_FWUpdate\_13.50.30.2154.exe" to the desktop*


2. Plug in the AC power.

**


3. Right-click on "AL156P1\_JL\_FWUpdate\_13.50.30.2154.exe" and run it as an administrator.

**


1. The User Account Control dialog box appears. Click *Yes* to continue.

**


1. The update ME dialog box appears. Click "Yes" to continue.

**

1. Warning: Firmware Update Required. It will display the current ME version and the new ME version. Click "Yes" to continue.



1. *Then update window will appear as below figure.*

**

*8.* After the FW update process is completed, the machine will automatically restart and enter the system.

9. After the update is completed, run the desktop"AL156P1\_JL\_FWUpdate\_13.50.30.2154.exe". A version check result pop-up window will appear.If the current ME version is the same as the version of the update package, it indicates that the FW update was successful; click OK to close the window.

