



ME&TPM Update and Check Steps  
  
Ensure that the battery power is > 25% before updating (need to connect AC adapter)

Steps  
1.Copy EXE to your desktop and run it as an administrator；  
  
  
  
  
EXE will run automatically, and the system will automatically restart after the completion of the run, and the update will be completed after the restart；  
  


2. ME & TPM Version Check  
Copy the CheckMEVersion folder to your desktop and double-click run.bat in the CheckMEVersion folder；

  
  
The figure below shows the running results, check that the ME version is 16.50.15.1515, and the TPM version is 600.18. 15.1515, and the update is successful。

ME version before update：16.50.0.1120，ME version after update：16.50.15.1515；  
TPM version before update：600.18.0.1120，TPM version after update：600.18. 15.1515；